**To check if ESP-32 is working, ran this code:**

int LED\_BUILTIN = 2;

void setup() {

pinMode (LED\_BUILTIN, OUTPUT);

}

void loop() {

digitalWrite(LED\_BUILTIN, HIGH);

delay(1000);

digitalWrite(LED\_BUILTIN, LOW);

delay(1000);

}